Pakistan Scientific & Technological Information Centre (PASTIC)
Pakistan Science Foundation (PSF)
Quaid-e-Azam University Campus, Islamabad 
P.O. Box: 1217, Islamabad, Tel: +9251-9248103-4, Fax: +9251-9248113, 
Email: dg@pastic.gov.pk, URL: www.pastic.gov.pk


INVITATION TO BID

Pakistan Scientific and Technological Information Centre a National Agency for collection and dissemination of scientific information invites sealed bids from the well-reputed Contractors/Builders registered with Income Tax and Sales Tax Departments ,Active Tax Payer (ATL) dealing in renovation/civil work for repair and maintenance of   PASTIC building at QAU,Islamabad.
2.	Bidding Documents, Containing detail Terms and Conditions may obtain at the office of Additional Director (Admin ) PASTIC QAU Campus, Islamabad during the office hours except gazetted holidays. Bidding documents can also be downloaded from the following websites.

a) www.ppra.org.pk   	(Public Procurement Regulatory Authority)
b) www.most.gov.pk 	(Ministry of Science and Technology)
c) www.psf.gov.pk 		(Pakistan Science Foundation)
d) www.pastic.gov.pk 	(Pakistan Scientific & Technological Information 
 			 	Centre (PASTIC)

[bookmark: _GoBack]3.	The bids, prepared in accordance with the instructions in the bidding documents, must reached at Pakistan Scientific & Technological Information Centre (PASTIC), National Centre, Q.A.U, Islamabad on 30/04/2018 at 11.00 a.m which will be opened on the same day at 2:00 pm in the presence of firms representative of the firm who may like to attend the Tender opening meeting.





Muhammad Ghazi
Additional Director ( Admin )
Ph.051-9248105

TENDER DOCUMENT

Name of Firm:			_________________________________
Address:			_________________________________
Telephone No:			____________Fax No. ______________
GST Reg. No.			_________________________________
National Tax Number:		_________________________________

	Sr. No.
	Description
	Qty.
approximately
	Rate
	Estimated cost

	
i.
	Item No. 1
Tiles Work In Library
Providing and lying floor comprising 2x2 China & Iran imported (Grade-A) superior quality non glazed tiles of approved shade set in neat Tile Bond cement paste not exceeding ¼” thick and filling the joint with neat white cement ¾” thick base in 1:3 cement and mortar laid over a bed (complete in all respect)
	
400-Sq.meter
	
-
	


	ii

	Fall Ceiling Work In Library
Providing and fixing of fall ceiling of 2’ x 2’ mineral fiber with T angle on imported fitting with proper leveling (complete in all respect.
	
2400 Sft
	
	



	iii.
	LED Lights in Library
Providing and Installation of LED lights(12 watts) with wiring 7/29 GM cable and switch fitting (complete in all respect).
	
80 Nos
	
	

	iv.
	Renovation of Bathrooms of Library side
Providing and lying of floor and walls(7ft height) tiles comprising China & Iran imported (Grade-A) superior quality of approved shade set with neat white cement ¾” thick base in 1:3 cement and mortar laid over a bed and dismantling the existin g tiles, proper pluming/electric work, replace of GI pipe and PVC pipe, painting on walls/roof,  providing and fixing of Porta English and Indian  seat, Sanitary set / (Muslim shower,Vanity marble(3’.6”x3’), two basin (Porta) mixer steel(Master). washroom accessories set(Master) (complete in all respect).
	ExisExisting Bathroom Lump sum
	
	

	v.
	
Construction of New Bathroom

Construction of  New baths room complete including (removing of existing wall) wall  partition of both bath room, RCC roof with the work of burnt brick masonry work, plaster work, paint work, walls tiles comprising China & Iran imported (Grade-A) superior quality of approved shade set with neat white cement ¾” thick base in 1:3 cement and mortar laid over a bed tiles work, fixing of Porta English and Indian  seat, Sanitary set, GI pipe and PVC pipe  (Muslim shower, Vanity marble (3’.6”x3’),  WC, pedestal, Basin, mixture, G.I. pipe, doors, chokhat, exhaust, PVC,  proper plumbring,Electric work. Washroom accessories (Complete in all respect).  
	
2-Nos 
150 sqft,
Approximately
Lump sum
	
	

	vi.
	Dismantling and Reconstruction of Wall of Library
Dismantling of existing 4” thick brick wall and shifting the dismantled material from the site at approved place and reconstruction of wall  with 4” brick cement 1: 4 plaster with masonry work (complete in all respects)
	 270-FT dismast
110-FT reconstruct

	
	

	vii.
	WHITE WASH IN LIBRARY
Two coats of plastic emulsion paint white and Half Color ICI, BUXLY, BERGER or Equivalent on and internal walls of PASTIC building including the cost of cleaning, scrabbling, filling, the surface and papering. (Complete in all respect.)
	5000-SFT
	
	

	      
   ITEM NO.02


	Viii.
	Glass Partition in Library and door
Providing and fixing of  Glass partition  with  12-mm Glass,D-48 Aluminium, and 2 -  auto doors  12-mm Glass with Aluminium, locks, steel handles, 2- motors  along with all  (superior quality) Taiwan/China Made (Complete in all respect)    
	300 -SFT
	
	

	ix.
	Library Terrace Gate
 Providing and fixing of (3- fixed  and 3- sliding)  5-mm Glass with silver Aluminium 16mm D48A sliding door with locks, silver handles (superior quality) Taiwan/China Made (Complete in all respect)    
	130-SFT
	
	

	x.
	Fish aquarium in Library,
 Providing and fixing of water cleaning motors with filter, Air pipes, ventilation pipe, marbles chips in basement, water plants, back scenery, wooden roofs, electric lights fish etc.
 Size: 10’x3”,10’x3”,10’x1’.5”x6’x1’.5”&3’x1’.3”
(Complete in all respect)
	lump sum
	
	

	Total
	
	
	-



TERMS & CONDITIONS
· Firms should quote their rates inclusive of all taxes as per (BOQ) after visiting the site.
· The bids will be evaluated in terms of the prescribed specifications/BOQ and lowest cost basis.
· Contract will be awarded to the firm or firms on the item wise lowest cost basis where as complete work is comprises on 02 items, work mentioned at Sr. No. i to vii will be treated as a part of item No. 01 and from viii to x is the part of item No. 2.

· The Firm mentioned its NTN and GST Numbers in their quotation and should be appeared on Active Tax pay List (ALT).
· Bid security equal to 5% of the total value of bid in shape of PO/DD in F/o PASTIC National Centre, Islamabad must be attached with the quotations.
· No bid will be accepted without bid security.
· The Job must be executed at PASTIC site located at Quaid-e-Azam University Campus, Islamabad, and completed within 60 days after issuance of work order.
· No transportation and carriage/mobilization charges will be allowed.
· Income tax will be deducted at source as per Government rules.
· The work done if found below standard/specifications will not be accepted and the Firm will have to do it again at his own risk and cost till the satisfaction of Inspection Team.
· Payment (100%) will be released on the satisfactorily completion of work.
· If the Firm found non Active Tax-Payer, his payment will be stopped till he files his mandatory returns and appears on ATL of FBR.
· All removal work will be done by the successful bidder before execution of renovation or construction.
· Rates must be valid for 90-days.


· Signature and seal of the Bidder






ACCEPTANCE CERTIFICATE


I ________________________________________________owner/representative of 
M/s ________________________________________, hereby, confirm that terms & conditions mentioned in this Tender Document are acceptable to me (as a whole) and I shall abide by these terms and conditions.

2.	The ____________________________________ as per specifications mentioned in the Tender Documents. I will be bound to replace any item, if found sub-standard, unsatisfactory or defective without any extra claim to PASTIC, Islamabad. If I failed to do so, I agree that PASTIC has the right to confiscate/forfeit the earnest money and May likely blacklist of our Firm.


(Supplier)



Signatures with seal:
(Owner/representation) 
Date__________

CNIC No. With attested copy___________________________________

Phone No___________________________
Cell No_____________________________
Fax No_____________________________


BILL OF QUANTITIES (BOQ )

	Sr. No.
	Description
	Qty.
	Rate
	Estimated cost

	
1.
	
Providing & Fixing Aluminum Doors

Providing and fixing sliver aluminum doors with milky glass for bathrooms 2.5x6.5 (complete in all respect)16.5@750 each14500
	8
	14500
	116000

	
2
	
Tiles Work In Committee Room

Providing and lying floor comprising 2x2 Pakistani, China & Iran (Grade-A) superior quality non glazed skid free tiles of approved shade set in neat Tile Bond cement paste not exceeding ¼” thick and filling the joint with neat white cement ¾” thick base in 1:3 cement and mortar laid over a bed
	 90 Meter 
	1600
	144000

	3
	
WHITE WASH OF  PASTIC BUILDING
Two coats of weather resistance paint (weather shield) white and Half Color ICI, BUXLY, BERGER or Equivalent on external and internal rooms walls, Oil paint on Doors and Grills of PASTIC building including the cost of cleaning, scrabbling, filling, the surface and papering and also the cost of scuff-folding where required at any height both sides front & back. (Complete in all respect.)
	9000sft 
	15
	135000

	
	395000


Quantity of the above work is subject to increase/decrease as per actual measurement work done at site








BILL OF QUANTITIES (BOQ)

	Sr. No.
	Description
	Qty.
	Rate
	Estimated cost

	
1.
	
Providing & Fixing Aluminum Doors

Providing and fixing silver aluminum doors with milky glass for bathrooms 2.5x6.5 (complete in all respect)
	8
	
	

	
2
	
Tiles Work In Committee Room

Providing and lying floor comprising 2x2 Pakistani, China & Iran (Grade-A) superior quality non glazed skid free tiles of approved shade set in neat Tile Bond cement paste not exceeding ¼” thick and filling the joint with neat white cement ¾” thick base in 1:3 cement and mortar laid over a bed
	 90 Meter 
	
	

	3
	
WHITE WASH OF  PASTIC BUILDING
Two coats of weather resistance paint (weather shield) white and Half Color ICI, BUXLY, BERGER or Equivalent on external and internal rooms walls, Oil paint on Doors and Grills of PASTIC building including the cost of cleaning, scrabbling, filling, the surface and papering and also the cost of scuff-folding where required at any height both sides front & back. (Complete in all respect.)
	9000sft 
1-4000sft
(weather shield)
2-3000sft
(Distemper)
3-2000sft
(Enamel Paint)

	
	

	
	


Quantity of the above work is subject to increase/decrease as per actual measurement work done at site





BILL OF QUANTITIES ( BOQ )

	Sr. No.
	Description
	Qty.
	Estimated cost

	1.
	Providing & Fixing Aluminum Doors

Providing laying and applying PA-3 water proofing pastorate econotop PA-3, modified bituminous membrane torch applied ploy merized containing nonwoven polyester coated on both side with pp modified bitumen compound having upper lower surface with polyethylene film and applying 3+04 sqm per liter on RCC surface roof and unrolling including the cost of removing scrapping mortar etc from the roof  surface disposing at scraped material debris and removing the dust by washing with water and removing the undulations, complete as per direction of Engineer inchage.
	11500sft or (as per actual)
	

	2
	TILES WORK IN COMMITTEE ROOM
Providing and lying floor comprising 2x2 Pakistani, China & Iran (Grade-A) superior quality non glazed skid free tiles of approved shade set in neat Tile Bond cement paste not exceeding ¼” thick and filling the joint with neat white cement ¾” thick base in 1:3 cement and mortar laid over a bed
	 90 Meter 
	




	3
	WHITE WASH OF  PASTIC BUILDING
Two coats of weather resistance paint (weather shield) white and Half Color ICI, BUXLY, BERGER or Equivalent on external and internal rooms walls, Oil paint on Doors and Grills of PASTIC building including the cost of cleaning, scrabbling, filling, the surface and papering and also the cost of scuff-folding where required at any height both sides front & back. (Complete in all respect.)
	9000sft 
	

	
	


Quantity of the above work is subject to increase/decrease as per actual measurement work done at site


BILL OF QUANTITIES ( BOQ )


	S. No
	Description
	Quantity 
	Rate 
	Amount 

	1.

	Providing and lying floor comprising 16x16 Master made superior quality non glazed skid free tiles of approved shade set in neat cement paste not exceeding ¼” thick and filling the joint with neat white cement salry using matching coloring ¾” thick base in 1:3 cement and mortar laid over a bed of 1 ½ thick (1:2:4) cleaning and curing etc complete at any floor at any height as directed. 
	450 Sft
	
	



BILL OF QUANTITIES ( BOQ )

	
S. No
	Description
	Qty
	Unit
	Rate
	Amount

	1.
	Two coats of weather resistance paint (weather shield) white and Half Color ICI, BUXLY, BERGER or Equivalent on external and internal rooms walls, Oil paint on Doors and Windows of PASTIC building including the cost of cleaning, scrabbling, filling, the surface and papering and also the cost of scuff-folding where required at any height both sides front & back and two water tank on building minor repair with cement, etc.( complete in all respect.) 
	9000Sft  
Approx.
	Per Sq.Ft
	
	

	TOTAL
	 






BILL OF QUANTITIES ( BOQ )




	S. No
	Description
	Qty
	Unit
	Rate
	Amount

	1.
	Color of PASTIC building with weather shield (white in color) both side of PASTIC building front & back and two water tank on building minor repair with cement, etc. complete in all respect. 
	8800Sft  
	Per Sq.Ft
	
	

	TOTAL
	 





BILL OF QUANTITIES ( BOQ )

	
S. No
	Description
	Qty
	Unit
	Rate
	Amount

	1.
	Two coats of weather resistance paint (weather shield) white Color ICI, BUXLY, BERGER or Equivalent on external walls of PASTIC building including the cost of cleaning, scrabbling, filling, the surface and papering and also the cost of scuff-folding where required at any height both sides fronts ( complete in all respect.) 
	6600Sft  
Approx.
	Per Sq.Ft
	
	

	TOTAL
	 





BOQ 
PASTIC Science and Reference Library Hall Fitting of Venial Tiles and other works  

	S. No
	Description
	Quantity 
	Rate 
	Amount 

	1.

	1.     Providing and fixing of new venial tiles.
I. Repair and re-fixing of old tiles
II.  Repair of Floor 
III. Cleaning/washing total Hall 
Complete in all respect  
	500 Sft
400 Sft
500 Sft
Lump sum 
	
	


























	S. No
	Description
	Quantity 
	Rate 
	Amount 

	1.

	1.     Providing and fixing of new venial tiles.
I.  Repair of Floor 
II. Cleaning/washing total Hall 
Complete in all respect  
	83- Meter
83- Meter
83- Meter
Lump sum 
	
	



( BOQ )


	S. No
	Description
	Quantity 
	Rate 
	Amount 

	1.

	Time Attendance Solution with X628-C Multimedia Fingerprint Time Attendance Terminal. 
	
	
	



BILL OF QUANTITIES ( BOQ )


	S. No
	Description
	Quantity 
	Rate 
	Amount 

	1.

	Providing and lying floor comprising 16x16 Master made superior quality non glazed skid free tiles of approved shade set in neat cement paste not exceeding ¼” thick and filling the joint with neat white cement salry using matching coloring ¾” thick base in 1:3 cement and mortar laid over a bed of 1 ½ thick (1:2:4) cleaning and curing etc complete at any floor at any height as directed. 
	450 Sft
	
	







The Additional Director (A&F)
PASTIC National Centre, 
Islamabad

QUOTATION 



	S. #
	Description
	Qty.
	Rate
	Amount 

	1.

	Providing and lying dress level finish and cure etc flooring in Tufftiles 2” thick in approved designe and color laid over a bed of sand about 1” thick filling the joint with sand compacting with viberator, filling the sites with concrete (1:2:4) complete in all respect.  
	1300Sft.
	Rs.65/-
	Rs.78,000/-


(Rupees seventy eight thousand only)




AKBAR ALI
QUOTATION



	S. No
	Description
	Rate

	1.

	Providing and lying dress level finish and cure etc flooring in Tufftiles 2” thick in approved designe and color laid over a bed of sand about 1” thick filling the joint with sand compacting with viberator, filling the sites with concrete (1:2:4) complete as directed.  
	70Sft.



QUOTATION



	S. No
	Description
	Quantity 
	Rate
	Amount

	1.

	Fencing of Iron gaze link 10 gages of 3x3'' centre of hole fixed on pole with clamps 5 on each pole fixed with pcc (124) two coats of enamel paint ici burger any color at East and North side of PASTIC building (University Huts)Complete in all respect.
	1800squft
	50
	Rs.90,000/-

	Total:-
	Rs.90,000/-


(Rupees ninety thousand only)





MUHAMMAD RAFI





BILL OF QUANTITIES ( BOQ )




	S. No
	Description
	Quantity 
	Rate
	Amount

	1.

	Fencing of Iron ghaze link 10 gage of 3x3'' centre of hole fixed on pole with clamps 5 on each pole at East and North side of PASTIC building (University Huts). Complete in all respect.
	1800squft
	43
	Rs.77,400/-

	Total :-
	Rs.77,400/-


(Rupees seventy seven thousand four hundred only)

 The Deputy Director
PASTIC Islamabad. 
 
Subject:	BILL OF QUANTITIES 




	S. #
	Description
	Qty
	Unit
	Rate
	Amount

	1.
	providing and fixing of MS Pipe Grills for ground floor (Reprographic Unit) of back side of PASTIC Building with 1/2x1/2 MS pipe of 18 gauge reference of PASTIC store fixed (subject to actual measuring) in brick wall windows with red oxide and black paint complete in all respect.   
	Complete job as per specification 
	75 sft
	250
	18750/-

	TOTAL
	18750/- 




BILL OF QUANTITIES ( BOQ )




	S. No
	Description
	Qty
	Unit
	Rate
	Amount

	1.
	Colour of PASTIC building with weather shield (white in colour) both side of PASTIC building front & back and two water tank on building minor repair with cement, etc. complete in all respect. 
	8800Sft  
	Per Sq.Ft
	
	

	TOTAL
	 





BILL OF QUANTITIES ( BOQ )




	S. No
	Description
	Qty
	Unit
	Rate
	Amount

	1.
	Providing/fitting of 18 gauge iron grills 2/4x2/4 solid bar, paining with red oxide and sliver colour in back side of PASTIC National Science Reference Library windows.
	332 Sft  
	Per Sq.Ft
	
	

	TOTAL
	 








BILL OF QUANTITIES ( BOQ )

	S. No
	Description
	Qty
	Unit
	Rate
	Amount

	1.
	Providing and fixing of fence 5 ft high around the PASTIC building post pipe 1-1/2 x 1-1/2 inch at the center of 4 ft expanded metal frame size 4’x2-1/2 ft pipe 18 gauge.
	1000 Sft  
	Per Sq.Ft
	
	

	2.
	Fabrication and fixation of motor vehicles shed in the PASTIC premises made of steel corrugated sheets and angle iron (Standard size) with two coats of paint.
	1800 Sft
	Per Sq.Ft
	
	

	3.
	Providing and lying tough tiles (superior quality) in front of Pastic main entrance
	1500 Sft
	Per Sq.Ft

	
	

	4.
	Seepage treatment of office toilets including replacement of defective pipes/fitting wherever required and floor tiling.
	Complete Job
	Complete Job
	
	

	5.
	Providing and fixing of grill inside made of MS pipe 1’’x1/2’’ outer frame section and inside ½ x ½ inch square pipe with 16 SWG gauge. ( First floor )
	500 Sft
	Per Sq.Ft

	
	

	6.
	Providing and fixing Electric Gyzer 10 Gallon Atlas/Singer/Toshiba or equivalent in toilets.  
	03 Nos
	Each
	
	

	TOTAL
	 








Signature of bidder with Seal.

BOQ 

Purchasing of floor Tiles For PASTIC Committee Room

	S. No
	Description
	Quantity 
	Rate 
	Amount 

	1.

	Providing new floor tiles.(16”x16”) Master, Shabbir Irani ,China or equivalent 
	68- Meter

	Rs.1175
	Rs.79900/-


                      (Rupees. Seventy nine thousand nine hundred eighty only)
BILL OF QUANTITIES ( BOQ )

	
S. No
	Description
	Qty
	Unit
	Rate
	Amount

	1.
	Two coats of weather resistance paint (weather shield) white Color ICI, BUXLY, BERGER or Equivalent on external walls of PASTIC building including the cost of cleaning, scrabbling, filling, the surface and papering and also the cost of scuff-folding where required at any height both sides front & back and two water tank on building minor repair with cement, etc.( complete in all respect.) 
	9000Sft  
Approx.
	Per Sq.Ft
	
	

	TOTAL
	 





